{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Faq"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Faq","index":0,"n_rows":2,"n_cols":3,"rows_kept":2,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["N.ro","Domanda","Risposta"]
[1,"In riferimento al Capitolato Speciale d’Appalto, relativamente alle caratteristiche minime richieste per la centrifuga a pag. 32, chiediamo cortesemente la possibilità di offrire un angolo di conicità tamburo ≤ 15° invece che ≤ 13°.\r\nQuesto senza compromettere le prestazioni minime richieste.\r\n","Pur trattandosi di un aspetto particolarmente delicato nella scelta e configurazione di un idroestrattore, si ritiene di poter accogliere la Vs richiesta purchè nell'offerta tecnica venga fornita adeguata documentazione a comprova della bontà/miglioria dell'angolo di conicità. La qualità della proposta sarà comunque verificata in sede di prova (così come previsto dall'art. 51 del CSA)."]